/*!
    \file  readme.txt
    \brief description of the USB Custom HID device demo
*/

/*
    Copyright (C) 2017 GigaDevice

    2017-02-10, V1.0.0, firmware for GD32F30x
*/

  This demo is based on the GD32F30x-EVAL board, it provides a description of 
how to use the USBFS.

  The GD32 device is enumerated as an USB Custom HID device, that uses the 
native PC Host HID driver.

  To test the demo, you need to:
    - Download the "Custom_HID Client" PC applet

    - Start the "Custom_HID Client" PC applet and connect GD32 USB to PC

    - The device should be detected and shown in the PC applet

    - Make sure that following report ID are configured: LED1 ID (0x11),
      LED2 ID(0x12), LED3 ID(0x13), LED4 ID(0x14), BUTTON1_ID(0x15) and
      BUTTON2_ID(0x16).

    - Select Leds in the applet to switch on/off on the EVAL board

    - Press the Wakeup key and Tamper key on the EVAL board to switch on
      /off the button1/button2 status in the PC applet