/*!
    \file  readme.txt
    \brief description of the ADC discontinuous mode example
*/

/*
    Copyright (C) 2017 GigaDevice

    2017-02-10, V1.0.0, firmware for GD32F30x
*/

  This demo is based on the GD32F30x-EVAL board, it shows how to use the
ADC discontinuous mode. The ADC is configured in discontinuous mode, group
length is 8, conversion length is 3, using software trigger. Every trigger 
converts 3 channels.

  You can use the watch window to see the conversion result.
  